[Models Supported] All the Rigol MSO8000 series oscilloscopes
[Latest Revision Date] 2025/03/21

[Notice] This firmware does NOT support the MSO8000A models. For those models, visit the official website of Rigol.

[Updated Contents]
Note: Before powering on the oscilloscope, ensure that the HDMI interface is disconnected. 


v00.02.03.00.00  2025/03/21
      - Modified the trigger sensitivity coefficient.

v00.02.02.00.01 2024/05/30
     -Added compatibility for PVA8150S probe
     -Added compatibility for PIA1050 and other opto-isolated probes

v00.01.02.00.07  2021/12/22

     - Added Averaging operation to the MATH function
     - Supported setting memory depth in the condition when the oscilloscope is in the STOP state
     - Added CAN-FD protocol decoding (MSO8000-AUTO option)
     - By default, in Zoom mode, "Zoom" is selected as the region for cursor measurement. A command relating to this function is also added. 
     - Added the function of modifying the channel label contents and the related SCPI commands
     - Added channel label font size setting and related SCPI command
     - Added channel label position setting and related SCPI command
     - Added command to switch the type of measurement threshold
     - Delay and phase measurements support setting the type of edge event
     - Modified the numeric keypad for cursor setting, added time and voltage units
     - Fixed the X cursor and Y cursor measurement errors in XY mode
     - Fixed the problem that the probe ratio did not work for the threshold setting in Search function
     - Fixed the decode error that occurs when polarity is Negative for Parallel decoding 
     - Fixed the problem that the RP7000 probe cannot be stably recognized when inserted
     - Fixed the risetime measurement error (Absolute threshold) when vertical offset is modified
     - Fixed the display dislocation of event table for RS232 decoding
     - Fixed the problem of displaying decimals for the totalizer
     - Math operation can turn off the display of signal source and only keep math waveform
     - Optimized the self-tuning algorithm and shorten the self-tuning time
     - Updated touch screen driver
     - Improved WebControl web page refresh speed (related to network speed)
     - Optimized WebControl web page control, supports dragging and drawing rectangles with the mouse
     - Supported modifying labels and file names through the physical keyboard
     - Optimized bandwidth frequency response @1MΩ input impedance
     - Supported the connection communication of T2R1000 probe adapter
     - Optimized the digital filtering function in math function
     - Optimized the display size of windows such as search lists
     - Optimized the display windows such as measurement, cursor, search and decoding event table, and support transparent background display
     - Optimized the manual cursor measurement function and support dual source measurement
     - Solved the problem of network printer printing failure


v00.01.01.00.00   2019/ 08/ 06

-Released the production version, updated LOGO
