This documentation is designed to provide guidance to customers on how to 
upgrade the DG5000 Pro series function / arbitrary waveform generator to the version in the 
"DG5000Pro(ARM)update.rar" file. 

 
New versions of firmware are available at the following website:
https://www.rigol.com/products/DG_detail/DG5000_Pro

[Notices]

    - Before upgrading, please carefully refer to the 
      "DG5000 Pro Release Notes.txt" file to obtain the updated information of
      the firmware version. 
      
    - Please make sure your USB disk can be read correctly. DG5000 Pro series 
      is required to use a USB Flash drive disk with FAT32 format. 
      
    - During the upgrade process, please do not cut off power and pull out the 
      USB disk, otherwise the instrument will fail to work normally.
       

[Upgrading Procedures]

    1. Copy the upgrade file DG5000ProUpdate.GEL to the root directory of the USB
       disk. 
       
    2. Keep the instrument in the power-on state, then insert the USB disk into
       the USB HOST interface (next to the Power key). 
       
    3. Enter the Storage module from left-down entry，select the Upgrade tab，click the path
        and select the package from USB disk. OK to start
       
    4. During the upgrade, the instrument interface will display the current 
       upgrade progress. 
       
    5. After upgrading has been completed, the instrument will restart. 
    
    6. Check whether the firmware version number has been updated 
       (press Utility -> About). 
       

[Troubleshooting]

    - If the instrument failed to read the upgrade file from the USB disk, 
      please try to replace the USB disk. 
      
    - If the problem still persists, please try to re-download the upgrade file.
    
    - If the problem still persists after performing the above two operations, 
      please visit the website int.rigol.com to find contacts in your area. 