[Model Supported] All the MSO8000A series oscilloscopes
[Latest Revision Date] 2023/08/14
[Updated Contents]
Note: When the oscilloscope is launched, ensure that the HDMI interface is disconnected. 

v00.03.01.00.00  2023/08/14
      - Enhanced functionality support for PVA8 series probes.


v00.03.00.00.06  2023/02/06
     - High resolution and BW is 3G  version

v00.01.02.00.07  2021/12/22

     - Added Averaging operation to the MATH function
     - Supported setting memory depth in the condition when the oscilloscope is in the STOP state
     - Added CAN-FD protocol decoding (MSO8000-AUTO option)
     - By default, in Zoom mode, "Zoom" is selected as the region for cursor measurement. A command relating
 to this function is also added. 
     - Added the function of modifying the channel label contents and the related SCPI commands
     - Added channel label font size setting and related SCPI command
     - Added channel label position setting and related SCPI command
     - Added command to switch the type of measurement threshold
     - Delay and phase measurements support setting the type of edge event
     - Modified the numeric keypad for cursor setting, added time and voltage units
     - Fixed the X cursor and Y cursor measurement errors in XY mode
     - Fixed the problem that the probe ratio did not work for the threshold setting in Search function
     - Fixed the decode error that occurs when polarity is Negative for Parallel decoding 
     - Fixed the problem that the RP7000 probe cannot be stably recognized when inserted
     - Fixed the risetime measurement error (Absolute threshold) when vertical offset is modified
     - Fixed the display dislocation of event table for RS232 decoding
     - Fixed the problem of displaying decimals for the totalizer
     - Math operation can turn off the display of signal source and only keep math waveform
     - Optimize the self-tuning algorithm and shorten the self-tuning time
     - Updated touch screen driver
     - Improved WebControl web page refresh speed (related to network speed)
     - Optimized WebControl web page control, supports dragging and drawing rectangles with the mouse
     - Supported modifying labels and file names through the physical keyboard
     - Optimized bandwidth frequency response @1MΩ input impedance
     - Supported the connection communication of T2R1000 probe adapter
     - Optimized the digital filtering function in math function
     - Optimized the display size of windows such as search lists
     - Optimized the display windows such as measurement, cursor, search and decoding event table, and 
support transparent background display
     - Optimized the manual cursor measurement function and support dual source measurement
     - Solved the problem of network printer printing failure


v00.01.01.00.00   2019/ 08/ 06

-Released the production version, updated LOGO