[Model Supported]  DSA705，DSA710，DSA815， DSA815-TG
[Latest Revision Date] 2016-09-26

[Updated Contents]

V00.01.19    2018-04-11

-----Solve the problem of LAN remote command timeout after opening 3 traces.
-----Modify the trace type for video avergage and power average.
-----Some other bug have been solved       


[Previous Versions and Updated Contents]

V00.01.18    2016-09-26

-----Reslove Ultra Spectrum problem
-----Perfect the SSC fuction
-----From this version, 
      Do not support the downgrade operation, 
      If special need ,please contact RIGOL technical support
      
V00.01.17    2016-08-15

-----Added the SSC fuction
-----Cleared the LAN communication trouble
-----Resolve the front panel switch control problem

V00.01.16    2016-05-18

------Resolved the remote control command problem
----- Resolved the problem caused by saving csv data when the horizontal 
     axis is represented in log form
-----Resolved the activation code failure problem 


V00.01.15    2015-10-23

----- Added JPEG and PNG format for image saving
----- Added loading the CSV format correction file
-----Cleared the math result error in averaging the power
-----Cleared the LAN communication connection error 
-----Cleared the hops occurred to the tracking source output at 10 MHZ


V00.01.14   2015-06-19

-----Added saving and printing for the invert image
-----Added the screensnap command 
-----Resolved the problem concerning the printer
-----Cleared the remote command error for keypad locking 


V00.01.13    2015-02-12

-----Compatible with the 09 version hardware, assisting the neilsbed 
     test and production 
-----Able to automatically modify the filter shape when RBW is 1 MHZ 


V00.01.12     2014-10-15

----- Added the key locking function
----- Added traditional Chinese in the system language
-----Added the command of the remote access to status of the reference
---- Added the sanitation function


V00.01.11     2014-09-04

-----Resolved the problem concerning the display of X axis in log form


V00.01.10     2014-05-27

-----Added the frequency offset function
-----Added remote commands that enable the instrument to switch between 
     the local mode and remote mode 
-----Improved the quality of AM demodulation


V00.01.09     2013-11-18

------Upgraded hardware version V05
------Added the "reset and averaging" function for the trace
------Added the correct self-calibration function
------Resolved the problem of failing to program the calibration data remotely
------Resolved the crash problem caused by trace data reading


V00.01.08  2013-10-29

------Added Korean, Japanese, Portuguese, German, 
      and Polish to the system language 


V00.01.07  2013-04-28

------Resolved the problem of spending too long time for storage operation 
------Resolved the problem of interface operation failure when outrange 
      occurred to the input signal and gave a warning 


V00.01.06   2012-07-24

------Improved OBW and EBW algorithm 
------Resolved the inaccuracy problem when the Zerospan sweep time is 20us


V00.01.05   2012-06-01

------Added the editing function for the relative value of the limit line
------Resolved the problem occurred to some instruments: 
      when PA is on, a prompt message indicating the outrange will be displayed. 


V00.01.04   2012-04-01

------Added some remote commands
------Resolved the problem: when ATT is 0, PA is on, 
      the amplitude error measured is too big. 


V00.01.03   2012-02-23

------Resolved the problem of failing to identify the USB disk
------Resolved the problem: unable to start the instrument if you want to 
      restart the instrument during the upgrade process. 


V00.01.02   2012-02-14

------Resolved the problem: TG scans only once when RBW is less than 10 KHZ.  


V00.01.01   2011-12-10

------Released the software version officially


