This documentation is designed to guide customers to upgrade
DSA875,DSA875-TG,DSA832,DSA832-TG  spectrum analyzers 
to the software version of this compressed package. 

New versions of DSA series firmware are available at the following website:
http://int.rigol.com/Product/ProductLine/3


********************************************************************************
     Please be sure to carefully check the product system information
     and component version.Incompatible upgrade will cause serious problems, 
     such as a failure in starting the instrument. 

********************************************************************************


[Important Notices]
   
Applicable models and component versions: 
    ------ Embedded software version number: 00.01.00 and later
    ------ BOOT version number: 00.01.00 and later
    ------ Digital FPGA version number: 00.01 and later
    ------ RF FPGA version number: 00.01  and later
    ------ Main board version number: 00.01 and later


********************************************************************************
     Please be sure to carefully check the product system information 
     and component version. Incompatible upgrade will cause serious problems,
     such as a failure in starting the instrument. 

********************************************************************************

[Notices]

  - Before upgrading, press [System]→"Information" to obtain system information. 
  - Before upgrading, refer to the "DSA875&DSA832 Release Notes. txt" file 
    to obtain the updated information of the firmware version. 
  - Please make sure your USB disk can be read correctly. 
    Only the USB disk with the FAT32 format is supported. 
  - During the upgrade process, please do not cut off power 
    and pull out the USB disk, otherwise the instrument will fail 
    to upgrade or even be damaged. 


[Upgrade Procedures]
 
   1. Press [System]→"Information" to obtain system information. 
   2. Check the system information of the instrument for upgrade requirements. 
      If the instrument meets the requirements for upgrade, 
      perform the following procedures; if not, stop upgrading. 
   3. Copy the upgrade file to the root directory of the USB disk. 
   4. Keep the instrument in the power-on state, then insert the USB disk
      into the USB HOST interface (next to the Power key). 
   5. Press [Storage] on the front panel of the instrument. 
      Select the upgrade file in the USB disk, and press "Sys Update". 
   6. Then, the instrument starts to upgrade. During upgrading, 
      the instrument interface will display the current upgrade progress. 
   7. After upgrading is completed successfully, 
      pull out the USB disk and restart the instrument. 
   8. Check whether the instrument version has been upgraded successfully. 

[Troubleshooting]

   1. If the instrument failed to read the upgrade file from the USB disk, 
      please try to replace the USB disk. 
   2. If the upgrade fails due to misoperations during upgrading, 
      please try the following operations. 
        2.1 Insert the USB disk and then start the instrument. 
        2.2 While the instrument is starting, continuously press the 
            green key [Preset] on the top left corner of the front panel. 
            Press and hold the key until the process bar appears at the 
            bottom left corner of the screen. 
        2.3 Observe the process bar and wait for the upgrade to be completed. 
        2.4 After upgrading is completed successfully, 
            pull out the USB disk and restart the instrument. 
   3. If the problem still persists after performing the above operations, 
      please visit the website www.int.rigol.com to find contacts in your area. 

