[Model Supported]  DSG5000
[Latest Revision Date] 2024-04-26


[Updated Contents]

V00.01.00.00.02

------After shutdown and restart, multiple channels/all channels have abnormal signal output
------CH1 starts scanning, causing CH2 to have no output。
------Below 250MHz, the amplitude error is approximately 7dB。
------After completing the frequency calibration of the upper computer, the frequency of the DSG5000 firmware version deviates when the machine restarts, and the frequency calibration data is not saved。



[Previous Versions and Updated Contents]

V00.01.00.00.01

------Fix the problem of crash when setting some parameters
------Optimize file loading and saving。

V00.01.00.00.00

------Optimize HDMI display。
