[Model Supported] RSA5065N，RSA5065，RSA5032N，RSA5032，RSA3030N，RSA3030，RSA3045N，RSA3045、RSA3015N、RSA3015
[Latest Revision Date] 2024-07-04


[Updated Contents]


00.03.07.00.01
	-Official version

[Previous Versions and Updated Contents]
00.03.06.07.02
	-Add VNA mode s11 measurement for calibration data storage and reading
00.03.06.06.02
	-Optimizing RSA5000 with significant differences between scan time and set time

00.03.06.05.02
	-Add memory requirements for limit lines and amplitude correction settings to the power on settings and stored "status files"
	-Error issue returned by the limit line test command (CALCurate: LLINe1: FAIL?) in EMI mode

00.03.06.05.01
	-Web control touch screen not working
	-Resolve the issue of changing the version number field from 3 to fully displayed in the system information

00.03.06 SP4 2023-12-09

	-Resolve remote command scanning crashes

00.03.06

- Resolve the issue of clearing and scanning for crashes in EMI mode
- VSA mode cannot save CSV file
- Error reading back value through socket port
- SCPI Command Issues in EMI Mode
- When measuring adjacent channel power (ACP), it is necessary to automatically switch the detection type to mean effective value
- Read back noise power no instruction
-Calibration kit for VNA measurement using SMA ports
- Solving the problem of CSV file frequency storage accuracy only reaching thousands of bits


00.01.03

- Solve the GPSA noise related problems.
- Solve the software function related problems.
- Solve the SCPI related problems.
- Solve the option related problems.

00.01.01

- Solve the density mode related problems.
- Solve the RTSA noise related problems.
- Solve the SCPI related problems.
- Solve the option related problems.
