[Model Supported] All the Rigol RSA3000/RSA5000 series spectrum analyzers, excluding the RSA3000E models.
[Latest Revision Date] 2024-07-04

[Notice] This firmware does NOT support RSA3015E, RSA3015E-TG, RSA3030E or RSA3030E-TG. For those models, visit the official website of Rigol.


[Updated Contents]

00.03.07.00.01
	-Official version


[Previous Versions and Updated Contents]

00.03.06.07.02
	-Added VNA mode s11 measurement for calibration data storage and reading
00.03.06.06.02
	-Optimized RSA5000 with significant differences between scan time and set time

00.03.06.05.02
	-Added memory requirements for limit lines and amplitude correction settings to the power on settings and stored "status files"
	-Error issue returned by the limit line test command (CALCurate: LLINe1: FAIL?) in EMI mode

00.03.06.05.01
	-Web control touch screen not working
	-Resolved the issue of changing the version number field from 3 to fully displayed in the system information

00.03.06 SP4 2023-12-09
	-Resolved remote command scanning crashes

00.03.06
	- Resolved the issue of clearing and scanning for crashes in EMI mode
	- VSA mode cannot save CSV file
	- Error reading back value through socket port
	- SCPI Command issues in EMI Mode
	- When measuring adjacent channel power (ACP), it is necessary to automatically switch the detection type to mean effective value
	- Read back noise power no instruction
	- Calibration kit for VNA measurement using SMA ports
	- Solved the problem of CSV file frequency storage accuracy only reaching thousands of bits

00.01.03
	- Solved the GPSA noise related problems.
	- Solved the software function related problems.
	- Solved the SCPI related problems.
	- Solved the option related problems.

00.01.01
	- Solved the density mode related problems.
	- Solved the RTSA noise related problems.
	- Solved the SCPI related problems.
	- Solved the option related problems.
